|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Manufacturer** | **Product** | **Range** (l/min) | **Accuracy** (%) | **Supply** (V) | **Communication** | **Comment** | **Price** (€ ex. VAT) |
| Omron | [D6F-P0010A1](https://www.tme.eu/nl/details/d6f-p0010a1/stromingsmeters/omron/) | 0-1 | ±5% | 4.75-5.25 | 0.2-2.5V Analog |  | 60 |
| Omron | [D6F-01A1-110](https://www.tme.eu/nl/details/d6f-01a1-110/stromingsmeters/omron/) | 0 - 1 | ±3% | 10.8-26.4 | 1-5V analog |  | 109 |
| Omron | [D6F-02A1-110](https://nl.mouser.com/ProductDetail/Omron-Electronics/D6F-02A1-110?qs=pWf36BUtxBgZztbtPnRw8g%3D%3D) | 0 - 2 | ±3% | 10.8-26.4 | 1-5V analog |  | 115 |
| Honeywell | [AWM3300V](https://nl.farnell.com/honeywell/awm3300v/sensor-air-flow-1000sccm-25psi/dp/1470602) | 0 - 1 | ±1% | 8-15 | 1-5V analog | Max 1.7bar  Non-linear | 114 |